**Leaving a Message**

1. User dials extension
2. N rings are reached
3. Greeting prompt
4. User presses 1 to leave record a message

User may hang up or wait for timeout after recording message to exit